**Blink LED with delay**

* Connect ESP32 to PC via USB cable
* Open the arduino IDE & select right board & port
* Connect LED +ve terminal to digital IO pin(22)
* Connect LED -ve terminal to resistor & resistor other terminal to GND
* Turns on and off a LED connected to digital pin, with delay of 5 seconds