**Interfacing buzzer with ESP32**

* Connect ESP32 to PC via USB cable
* Open the arduino IDE & select right board & port
* Connect buzzer +ve terminal to digital IO pin(21)
* Connect buzzer -ve terminal to GND
* Turns on and off a buzzer connected to digital pin, with delay of 5 seconds